**1-scanner online measurement systems continuously monitor the basic parameters of the paper like basis weight, moisture, ASH & Caliper, porosity measurements, color interpretation, etc**.

Specification-

-Paper Grade & GSM Range with parameters

-Sole plate center.

-Width of the paper. -Heigh of the paper from sole plate.

-No of source is required .

-system software

**Motor-**

KW/ HP

RPM/POLE

FRAME SIZE

MOUNTING

Standard

Ambient temperature

Body enclosure

Duty

Enclosure

Insulation class

Ip degree of protection

Speciality

Phase

Terminal box location

Voltage

Frequency

**Drive**

Input power voltage/frequency

Output voltage/ frequency

Input Devices

Pwm carries frequency

Motor Requirement

Overload capacity

Start stop

Ambient condition

Enclosure

Maximum high voltage wire length

Compliance

CE

Dimensions

Weight

**Cable**

Application

Voltage Rating

Operating Temperature

Core Identification

Construction

**Pump**

Position

Liquid Handled

Consistency %

Specific Gravity

Temperature in Deg C

PH value

Capacity cum/hr

Head in mtrs

Type of impeller

Motor required

Efficiency in%

MOC

Type of Gland/ mechanical seal

**Pipeline**

Pipe

-Stainless steel

-Grade

-Size

-Schedule

-Length

Elbow

-Grade

-Size

-Schedule

-Type (long,short)

Stub End

-Grade

-Size

-Schedule

-Type (long,short)

Certification for SS Milltest

MS & IBR

-Class

-Size

-Length

-Type

certification for MS mill test

**Foundation & Errection**

Scope

Errection of static equipment

Errection of Rottery equipment and machinery

Special instructions to contractor

Delivery storage & custody of equipment and machinery

Handing, Transporting, and Errection

Grouting

Final grouting check & finishing

Trial run of equipment & machinery

System Test/startup (precommissioning)

**Miscellaneous**-**freight & Escallation**

Providing Crain, Hydra for loading, unloading the material

providing necessary steel structure material

Providing necessary amenities

Providing consumable material

Providing rooms for Errection contractor labor