****

**⏵ANNEXURE-B**

**STANDARD FITTINGS & ACCESSORIES FOR 500 KVA DISTRIBUTION TRANSFORMER WITH BUILT- IN H.T. AUTOMATIC VOLTAGE REGULATOR**

**FITTINGS Unit-B Unit- A&C Make**

1. Ratting Plate 1 No. 1No. Globe
2. Earthing Terminals 2Nos. 2Nos. Globe
3. Bi-Directional Roller 4 Nos. 4 Nos. Globe
4. Lifting Lugs 2 Nos 2 Nos. Globe
5. Drain Valve cum Button filter valve with plug 1 No. 1 No. Globe
6. Top Filter valve with plug Nil 1 No. Globe
7. Silicagel Breather 1 No. 1 No. TEMP
8. Inspection Cover Nill. 1 No. Globe
9. Air Release Plug Nil As Per Req. Globe
10. Pressed Steel Radiators As per Req. As per Req. Any Standard Make
11. Radiator Valves do do. Hari
12. Buchholz Relay Nill. 1 No.
13. Buchholz Relay Shut Off Valve Nill. 1 No.
14. Conservator fitted with Oil filling Hole & Drain Plug Nill. 1 No. Globe
15. Plain Oil Level Gauge 1No. 1No. Globe
16. OTI with A/T Contacts Nill. 1 No. TEMP
17. P.T. for Output Voltage Measurement & sensing CKT Nill. Used as regulator

Voltage Ratio /output Voltage

1. Marshalling Box Nill. 1 No. Globe
2. Step Syn Geared Motor Torque 20Kg 1No. Nill. Uni-Step
3. Explosion Vent Nilll. 1No. Globe

Unit ‘D’ : AUTOMATIC CONTROL PANEL COMPRISING THE FOLLOWING

1. Sensing Controlled CKT 2 No. Globe Make
2. Calibrated Voltmeter for Output Measurement 1 No. Any standard Make
3. Voltage Adjustment Accessories 1 No. Pankaj
4. Inc. / Dec. Arrangement 1 No. Kay Cee Make
5. Auto/Manual Arrangement 1No. Kay Cee make