|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SR. NO** | **EQUIPMENT NAME** | **MANUFACTURER****NAME** |  **DETAILS** | **MANUFACTURING YEAR** |
| 1. | BOILER | SICHUANCHUANGUO BOILER CO. LTD , CHINA | .CAPACITY -230 TPH.RATEAD PRESSURE-9.80 MPA.RATED TEMPRATURE-540 ®C | 2011 |
| 2. | TURBINE | SHANDONG JINAN STEAM TURBINE. | .TYPE- STEAM CONDESING STEAM TURBINE.RATED RPM-3000.STAGES- 17.SURFACE TYPE STEAM CONDENSOR | 2011 |
| 3. | ID-1 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY | .POWER- 800KW.RATED SPEED-992RPM.CURRENT-87AMP.VOLTAGE-6600 V | 2011 |
| 4. | ID-1 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA | .FLOW RATE-284200m3/HR.RATED SPEED- 992RPM | 2011 |
| 5. | ID-2 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY. | .POWER- 800KWRATED SPEED-992 RPMCURRENT-87 AMP.VOLTAGE-6600 V | 2011 |
| 6. | ID-2 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA. | FLOW RATE-284200m3/HR.RATED SPEED- 992RPM. | 2011 |
| 7. | PA-1 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY. | OUTPUT-800KWSPEED-1490 RPMVOLTAGE-6600 VCURRENT-83 AMP. | 2011 |
| 8. | PA-1 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA. | .FLOW RATE-95110 m3/HR.RATED SPEED-1490 RPM | 2011 |
| 9. | PA-2 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY. | OUTPUT-800KWSPEED-1490 RPMVOLTAGE-6600 VCURRENT-83 AMP. | 2011 |
| 10. | PA-2 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA.. | .FLOW RATE-95110 m3/HR.RATED SPEED-1490 RPM. | 2011 |
| 11. | SA-1 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY. | OUTPUT- 630KWSPEED-1490 RPMCURRENT- 66 AMPVOLTAGE-6600 V | 2011 |
| 12. | SA-1 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA. | TYPE-CENTRIFUGAL FANFLOW RATE-129700 m3/HRRATED SPEED-1450RPM. | 2011 |
| 13. | SA-2 MOTOR | SHADONG JINAN POWEREQUIPMENT FACTORY. | OUTPUT- 630KWSPEED-1490 RPMCURRENT- 66 AMPVOLTAGE-6600 V. | 2011 |
| 14. | SA-2 FAN | JINAN VENTILATOR FACTORY CO. LTD OF CHINA. | TYPE-CENTRIFUGAL FANFLOW RATE-129700 m3/HRRATED SPEED-1450RPM. | 2011 |
| 15. | WALL SEAL MOTOR-1 |  | POWER -75KWVOLTAGE-415VCURRENT-128 AMP | 2011 |
| 16. |  BLOWER-1 |  |  | 2011 |
| 17. | WALL SEAL MOTOR-2 |  | POWER -75KWVOLTAGE-415VCURRENT-128 AMP. | 2011 |
| 18. | BLOWER-2 |  |  | 2011 |
| 19. | BFP-1 MOTOR | SIMO MOTORS ,CHINA | OUTPUT-1600KWVOLTAGE-6600VSPEED-2980 RPM | 2011 |
| 20. | BFP-1 PUMP | KSB INDIA PVT LTD |  | 2011 |
| 21. | BFP-2 MOTOR | SIMO MOTORS ,CHINA. | OUTPUT-1600KWVOLTAGE-6600VSPEED-2980 RPM. | 2011 |
| 22. | BFP-2 PUMP | KSB INDIA PVT LTD |  | 2011 |
| 23. | MCW -1 MOTOR | MARATHON ELECTRIC | OUTPUT-830KWVOLTAGE-6600 VCURRENT-91 AMPSPEED- 989 RPM | 2011 |
| 24. | MCW-1 PUMP |  |  | 2011 |
| 25. | MCW-2 MOTOR | MARATHON ELECTRIC | OUTPUT-830KWVOLTAGE-6600 VCURRENT-91 AMPSPEED- 989 RPM. | 2011 |
| 26. | MCW-2 PUMP |  |  | 2011 |
| 27. | MCW-3 MOTOR | MARATHON ELECTRIC. | OUTPUT-830KWVOLTAGE-6600 VCURRENT-91 AMPSPEED- 989 RPM. | 2011 |
| 28. | MCW-3 PUMP |  |  | 2011 |
| 29. | ACW-1 MOTOR | MARATHON ELECTRIC. | OUTPUT-250KWVOLTAGE-6600 VSPEED-1488 RPM | 2011 |
| 30. | ACW-1 PUMP |  |  | 2011 |
| 31. | ACW-2 MOTOR | MARATHON ELECTRIC. | OUTPUT-250KWVOLTAGE-6600 VSPEED-1488 RPM. | 2011 |
| 32. | ACW-2 PUMP |  |  | 2011 |
| 33. | TURBOGENERATOR | SHANDONG JINAN POWER EQUIPMENT FACTORY | RATED POWER -50MWRATED VOLTAGE-11000 VRATED SPEED-3000RPM |  |
|  |  |  |  |  |