|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SR. NO** | **EQUIPMENT**  **NAME** | **MANUFACTURER**  **NAME** | **DETAILS OF**  **EQUIPMENT** | **MANUFACTURING**  **YEAR** |
| 1. | BOILER | ISGEC HEAVY  ENGINEERING LTD. | 1).TYPE -CFBC Boiler,  2). CAPACITY-215 TPH,  3).WORKING PRESSURE & TEMP  -109 kg/cm2, 540 ®, 4).Total Heating Surface Area -18148 m2 | 2015 |
| 2. | TURBINE | BHEL | Steam Turbine, 3000 RPM, stages-49     , Extractions-04, Air cooled condenser. | 2015 |
| 3. | ID -1 MOTOR | ABB INDIA LTD | OUTPUT-530KW / 710HP  RPM-989  VOLTAGE-6600V  CURRENT-60 AMP | 2015 |
| 4. | ID-1 FAN |  | IMPELLER TYPE - CENTRIFUGAL, BACKWARD CURVED.  RPM- 990  TYPE OF DRIVE- CONSTANT SPEED | 2015 |
| 5. | ID-2 MOTOR | ABB INDIA LTD | OUTPUT-530KW / 710HP  RPM-989  VOLTAGE-6600V  CURRENT-60 AMP | 2015 |
| 6. | ID-2 FAN |  | IMPELLER TYPE - CENTRIFUGAL, BACKWARD CURVED .  RPM- 990  TYPE OF DRIVE- CONSTANT SPEED. | 2015 |
| 7. | PA-1 MOTOR | MARATHON | 560KW/751HP | 2015 |
| 8. | PA-1 FAN |  | IMPELLER TYPE- CENTRIFUGAL, BACKWARD CRVED  TYPES OF DRIVE- CONSTANT SPEED  SPEED -1490 RPM | 2015 |
| 9. | PA-2 MOTOR | CROMPTON GREAVES LTD. | 560KW/751HP  RPM- 1475 | 2015 |
| 10. | PA -2 FAN |  | IMPELLER TYPE- CENTRIFUGAL, BACKWARD CRVED  TYPES OF DRIVE-  CONSTANT SPEED  SPEED-1490 RPM | 2015 |
| 11. | SA -1 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-225KW/302HP  VOLTAGE-6600V  CURRENT-22AMP  SPEED-1485 RPM | 2015 |
| 12. | SA-1 FAN |  |  | 205 |
| 13. | SA-2 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-225KW/302HP  VOLTAGE-6600V  CURRENT-22AMP  SPEED-1485 RPM. | 2015 |
| 14. | SA-2 FAN |  |  | 2015 |
| 15. | WALL SEAL MOTOR-1 | CROMPTON GREAVES LTD. | OUTPUT-22KW  VOLTAGE-415V  CURRENT-40.5AMP | 2015 |
| 16. | WALL SEAL BLOWER-1 | SWAM PNEUMATIC PVT LTD. | FLOW-2200m3/HR  SPEED-900 RPM  PRESSURE-2500 MMWC. | 2015 |
| 17. | WALL SEAL  MOTOR-2 | CROMPTON GREAVES LTD | OUTPUT-22KW  VOLTAGE-415V  CURRENT-40.5AMP  . | 2015 |
| 18. | WALL SEAL  BLOWER-2 | SWAM PNEUMATIC PVT LTD. | FLOW-2200m3/HR  SPEED-900 RPM  PRESSURE-2500 MMWC | 2015 |
| 19. | CEP-1 MOTOR | ABB INDIA LTD | OUTPUT-180KW/240HP  CURRENT-293AMP  VOLTAGE-415V | 2015 |
| 20. | CEP-1 PUMP | KSB PUMP LTD | FLOW RATE- 192 m3/hr.  HEAD- 168 meter  SPEED- 2980 RPM. | 2015 |
| 21. | CEP-2 MOTOR | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 22. | CEP-2 PUMP | KSB PUMP LTD. | FLOW RATE- 192 m3/hr.  HEAD- 168 meter  SPEED- 2980 RPM | 2015 |
| 23. | ACW-1 MOTOR | MARATHO | OUTPUR-180KW/240HP  VOLTAGE-415V  CURRENT-310AMP  SPEED-1485RPM | 2015 |
| 24. | ACW-1 PUMP | MATHER AND PLATT PUMPS LTD | FLOW RATE-91 m3/hr  HEAD -91 METER  SPEED- 1485RPM | 2015 |
|  |  |  |  |  |
| 25. | ACW-2 MOTOR | MARATHON | OUTPUR-180KW/240HP  VOLTAGE-415V  CURRENT-310AMP  SPEED-1485RPM. | 2015 |
| 26. | ACW-2 PUMP | MATHER AND PLATT PUMPS LTD | FLOW RATE-91 m3/hr  HEAD -91 METER  SPEED- 1485RPM. | 2015 |
| 27. | BFP-1 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-1580KW/2118KW  VOLTAGE-6600V  CURRENR-158AMP  SPPED-2980 RPM | 2015 |
| 28. | BFP-1 PUMP | KSB PUMP LTD | FLOW RATE- 267 m3/hr | 2015 |
| 29. | BFP-2 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-1580KW/2118KW  VOLTAGE-6600V  CURRENR-158AMP  SPPED-2980 RPM. | 2015 |
| 29. | BFP-2 PUMP | KSB PUMP LTD | FLOW RATE- 267 m3/hr | 2015 |
| 30. | AOP MOTOR | CROMPTON GREAVES LTD. | OUTPUT-75KW/100HP  VOLTAGE-415V  CURRENT-124 AMP | 2015 |
| 31. | AOP PUMP | SULZER PUMP INDIA LTD | FLOW RATE-150 m3/hr  HEAD- 102 METER  SPEED -2970 RPM | 2016 |
| 32. | MOP MOTOR | CROMPTON GREAVES LTD.. | OUTPUT-75KW/100HP  VOLTAGE-415V  CURRENT-124 AMP  SPEED-2970RPM | 2015 |
| 33. | MOP PUMP | SULZER PUMP INDIA LTD | FLOW RATE-150 m3/hr  HEAD- 102 METER  SPEED -2970 RPM  . | 2015 |
| 34. |  |  |  |  |
| 35. |  |  |  |  |
| 36 | JOP-1 MOTOR  ( D.C) | CROMPTON GREAVES LTD. | OUTPUT- 18.5KW/25HP  V0LTAGE-110V  SPEED-1450RPM | 2015 |
| 37. | JOP-1 PUMP | TUSHACO PUMP PVT LTD. | SPEED-1450RPM  DISCHARGE PRESSURE-150 KG/cm2. | 2015 |
| 38. | JOP -2 MOTOR  (A.C) | CROMPTON GREAVES LTD.. | OUTPUT-18.5KW/25HP  VOLTAGE-415 V  CURRENT-34 AMP  SPEED-1475RPM | 2015 |
| 39. | JOP-2 PUMP | TUSHACO PUMP PVT LTD | SPEED-1450RPM  DISCHARGE PRESSURE-150 KG/cm2 | 2015 |
| 40. | EOP MOTOR  (D.C) |  | OUTPUT-75KW/100HP  SPEED-2930RPM |  |
| 40. | ACC MOTOR-1 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 41. | ACC MOTOR-2 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 42. | ACC MOTOR-3 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 43. | ACC MOTOR-4 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 44. | ACC MOTOR-5 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 45. | ACC MOTOR-6 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 46. | ACC MOTOR-7 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 47. | ACC MOTOR-8 | ABB INDIA LTD | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM | 2015 |
| 48. | ACC MOTOR-9 | ABB INDIA LTD. | OUTPUT-110/240HP  VOLTAGE-415V  CURRENT-186AMP  SPEED-1486 RPM  . | 2015 |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |