|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SR. NO** | **EQUIPMENT**  **NAME** | **MANUFACTURER****NAME** | **DETAILS OF** **EQUIPMENT** | **MANUFACTURING**  **YEAR** |
|  1. | BOILER |  ISGEC HEAVY ENGINEERING LTD. | 1).TYPE -CFBC Boiler,2). CAPACITY-215 TPH, 3).WORKING PRESSURE & TEMP-109 kg/cm2, 540 ®, 4).Total Heating Surface Area -18148 m2 |  2015 |
|  2. | TURBINE | BHEL | Steam Turbine, 3000 RPM, stages-49     , Extractions-04, Air cooled condenser. |  2015 |
|  3. | ID -1 MOTOR | ABB INDIA LTD | OUTPUT-530KW / 710HPRPM-989VOLTAGE-6600VCURRENT-60 AMP | 2015 |
|  4. | ID-1 FAN |  | IMPELLER TYPE - CENTRIFUGAL, BACKWARD CURVED.RPM- 990TYPE OF DRIVE- CONSTANT SPEED  | 2015 |
| 5. | ID-2 MOTOR | ABB INDIA LTD | OUTPUT-530KW / 710HPRPM-989VOLTAGE-6600VCURRENT-60 AMP | 2015 |
| 6. | ID-2 FAN |  | IMPELLER TYPE - CENTRIFUGAL, BACKWARD CURVED .RPM- 990TYPE OF DRIVE- CONSTANT SPEED. | 2015 |
| 7. | PA-1 MOTOR | MARATHON | 560KW/751HP | 2015 |
| 8. | PA-1 FAN |  | IMPELLER TYPE- CENTRIFUGAL, BACKWARD CRVEDTYPES OF DRIVE- CONSTANT SPEEDSPEED -1490 RPM | 2015 |
| 9. | PA-2 MOTOR | CROMPTON GREAVES LTD. | 560KW/751HPRPM- 1475 | 2015 |
| 10. | PA -2 FAN |  | IMPELLER TYPE- CENTRIFUGAL, BACKWARD CRVEDTYPES OF DRIVE- CONSTANT SPEEDSPEED-1490 RPM | 2015 |
| 11. | SA -1 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-225KW/302HPVOLTAGE-6600VCURRENT-22AMPSPEED-1485 RPM | 2015 |
| 12. | SA-1 FAN |  |  | 205 |
| 13. | SA-2 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-225KW/302HPVOLTAGE-6600VCURRENT-22AMPSPEED-1485 RPM. | 2015 |
| 14. | SA-2 FAN |  |  | 2015 |
| 15. | WALL SEAL MOTOR-1 | CROMPTON GREAVES LTD. | OUTPUT-22KWVOLTAGE-415VCURRENT-40.5AMP | 2015 |
| 16. | WALL SEAL BLOWER-1 | SWAM PNEUMATIC PVT LTD. | FLOW-2200m3/HRSPEED-900 RPMPRESSURE-2500 MMWC. | 2015 |
| 17. | WALL SEAL MOTOR-2 | CROMPTON GREAVES LTD | OUTPUT-22KWVOLTAGE-415VCURRENT-40.5AMP. | 2015 |
| 18. |  WALL SEAL BLOWER-2 | SWAM PNEUMATIC PVT LTD. | FLOW-2200m3/HRSPEED-900 RPMPRESSURE-2500 MMWC | 2015 |
| 19. | CEP-1 MOTOR | ABB INDIA LTD | OUTPUT-180KW/240HPCURRENT-293AMPVOLTAGE-415V | 2015 |
| 20. | CEP-1 PUMP | KSB PUMP LTD | FLOW RATE- 192 m3/hr.HEAD- 168 meterSPEED- 2980 RPM. | 2015 |
| 21. | CEP-2 MOTOR | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 22. | CEP-2 PUMP | KSB PUMP LTD. | FLOW RATE- 192 m3/hr.HEAD- 168 meterSPEED- 2980 RPM | 2015 |
| 23. | ACW-1 MOTOR | MARATHO | OUTPUR-180KW/240HPVOLTAGE-415VCURRENT-310AMPSPEED-1485RPM | 2015 |
| 24. | ACW-1 PUMP | MATHER AND PLATT PUMPS LTD | FLOW RATE-91 m3/hrHEAD -91 METERSPEED- 1485RPM | 2015 |
|  |  |  |  |  |
| 25. | ACW-2 MOTOR | MARATHON | OUTPUR-180KW/240HPVOLTAGE-415VCURRENT-310AMPSPEED-1485RPM. | 2015 |
| 26. | ACW-2 PUMP | MATHER AND PLATT PUMPS LTD | FLOW RATE-91 m3/hrHEAD -91 METERSPEED- 1485RPM. | 2015 |
| 27. | BFP-1 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-1580KW/2118KWVOLTAGE-6600VCURRENR-158AMPSPPED-2980 RPM | 2015 |
| 28. | BFP-1 PUMP | KSB PUMP LTD | FLOW RATE- 267 m3/hr | 2015 |
| 29. | BFP-2 MOTOR | CROMPTON GREAVES LTD. | OUTPUT-1580KW/2118KWVOLTAGE-6600VCURRENR-158AMPSPPED-2980 RPM. | 2015 |
| 29. | BFP-2 PUMP | KSB PUMP LTD | FLOW RATE- 267 m3/hr | 2015 |
| 30. | AOP MOTOR | CROMPTON GREAVES LTD. | OUTPUT-75KW/100HPVOLTAGE-415VCURRENT-124 AMP | 2015 |
| 31. | AOP PUMP | SULZER PUMP INDIA LTD | FLOW RATE-150 m3/hrHEAD- 102 METERSPEED -2970 RPM | 2016 |
| 32. | MOP MOTOR | CROMPTON GREAVES LTD.. | OUTPUT-75KW/100HPVOLTAGE-415VCURRENT-124 AMPSPEED-2970RPM | 2015 |
| 33. | MOP PUMP | SULZER PUMP INDIA LTD | FLOW RATE-150 m3/hrHEAD- 102 METERSPEED -2970 RPM. | 2015 |
| 34. |  |  |  |  |
| 35. |  |  |  |  |
| 36 | JOP-1 MOTOR( D.C) | CROMPTON GREAVES LTD. | OUTPUT- 18.5KW/25HPV0LTAGE-110VSPEED-1450RPM | 2015 |
| 37. | JOP-1 PUMP | TUSHACO PUMP PVT LTD. | SPEED-1450RPMDISCHARGE PRESSURE-150 KG/cm2. | 2015 |
| 38. | JOP -2 MOTOR(A.C) | CROMPTON GREAVES LTD.. | OUTPUT-18.5KW/25HPVOLTAGE-415 VCURRENT-34 AMPSPEED-1475RPM | 2015 |
| 39. | JOP-2 PUMP | TUSHACO PUMP PVT LTD | SPEED-1450RPMDISCHARGE PRESSURE-150 KG/cm2 | 2015 |
| 40. | EOP MOTOR(D.C) |  | OUTPUT-75KW/100HPSPEED-2930RPM |  |
| 40. | ACC MOTOR-1 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 41. | ACC MOTOR-2 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 42. | ACC MOTOR-3 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 43. | ACC MOTOR-4 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 44. | ACC MOTOR-5 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 45. | ACC MOTOR-6 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 46. | ACC MOTOR-7 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 47. | ACC MOTOR-8 | ABB INDIA LTD | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM | 2015 |
| 48. | ACC MOTOR-9 | ABB INDIA LTD. | OUTPUT-110/240HPVOLTAGE-415VCURRENT-186AMPSPEED-1486 RPM. | 2015 |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |